
### Difficult pairing

To pair the sensor it needs to be reset first, by pressing the pin-hole button for 10 seconds.

Then after starting sensor search, press the button again until the LED blinks.
Finally continuously press the button every 2 seconds until joining is confirmed.
